{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Planilha1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Planilha1","index":0,"n_rows":3,"n_cols":6,"rows_kept":3,"cut":false,"hidden":false,"merged":[[0,0,0,5]]}
["ANEXO I – ESPECIFICAÇÕES TÉCNICAS, QUANTITATIVOS E CUSTOS ESTIMADOS"]
["ITEM","CÓDIGO CATMAT","DESCRIÇÃO","QUANTIDADE (unidade)","VALOR UNITÁRIO (R$)","VALOR TOTAL (R$)"]
[1,619078,"Fornecimento, transporte, carga, descarga e instalação, na área de atuação da 11ª Superintendência Regional da Codevasf (Amapá), de Píer Flutuante em formato de “T” fabricado a partir da montagem de módulos plásticos, com dimensões mínimas de 50cm x 50cm x 35cm. Construído com material de Polietileno de Alta Densidade (PEAD). O Píer Flutuante deve atender uma área de 50m² divididas em duas partes: uma entrada com 10 m² (2 m x 5 m) e uma frente de 40 m² (20 m x 2 m). O píer deve contar com todo o aparato de segurança necessário ao seu funcionamento. Garantia mínima de 12 meses, contada a partir do recebimento definitivo do bem, atestado pelo fiscal. Com logomarca da Codevasf silkada.",16,null,{"$f":"D3*E3","v":0}]